

DATE ______________________________
                               SPRING WORK LIST




BOAT NAME________ ______________________________________________________________________________

LAUNCH/READY BY Date:_____________________________ S.S.M. Launch c Customer Pick up c

OUR STANDARD SPRING COMMISSIONING PROCEDURES INCLUDE:
	
	Maintenance of exterior wood specific to finish on your boat (if applicable) varnish/oil/clean

	
	Bottom paint

	
	Ensure all batteries are fully charged/install

	
	Zincs/Anodes Changed

	
	Rinse freshwater system (if applicable)

	
	Inspect and test electrical system (if applicable)

	        
	Inspect and test plumbing system (if applicable)

	
	Maintain seacocks (if applicable)

	
	Run and check engine

	
	Check safety equipment

	
	Clean, buff & wax hull

	
	Clean interior

	
	Reinstall any cushions/equipment/electronics removed from boat during storage

	
	Fill fuel tanks

	
	Launch

	
	Clean, commission and launch dinghy (if applicable)

	
	Change impeller

	
	Any Additional Comments:

	
	

	
	

	
	




Please check off all work to be completed by Stockton Springs Marine prior to spring commissioning.  If we do not hear back from you we will perform all of the above standard procedures.  We will touch base with you in April to see if there is any additional work you would like performed and to reconfirm your anticipated launch date.  Projects not on the list at that time cannot be guaranteed to be completed by launching.
All yard/storage bills must be paid in full prior to launch.

	CUSTOMER NAME
	CUSTOMER SIGNATURE



